Log CCU2: 
Dec 13 10:35:25 homematic-ccu2 syslog.info syslogd started: BusyBox v1.20.2                                                                                                                                                      
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: klogd started: BusyBox v1.20.2 (2015-10-16 10:11:13 CEST)                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] Booting Linux on physical CPU 0                                                                                                                                  
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] Initializing cgroup subsys cpu                                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000] Linux version 3.4.11.ccu2 (hudson@entw-build-10) (gcc version 4.6.1 (Sourcery CodeBench Lite 2011.09-70) ) #1 PREEMPT Fri Oct 16 10:43:35 CEST 2015            
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.000000] CPU: ARM926EJ-S [41069265] revision 5 (ARMv5TEJ), cr=00053177                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.000000] CPU: VIVT data cache, VIVT instruction cache                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.000000] Machine: eQ-3 HomeMatic CCU2                                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.000000] Memory policy: ECC disabled, Data cache writeback                                                                                                                
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    0.000000] On node 0 totalpages: 65536                                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    0.000000] free_area_init_node: node 0, pgdat c03b607c, node_mem_map c03ea000                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    0.000000]   Normal zone: 512 pages used for memmap                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    0.000000]   Normal zone: 0 pages reserved                                                                                                                                 
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    0.000000]   Normal zone: 65024 pages, LIFO batch:15                                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    0.000000] pcpu-alloc: s0 r0 d32768 u32768 alloc=1*32768                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    0.000000] pcpu-alloc: [0] 0                                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.000000] Built 1 zonelists in Zone order, mobility grouping on.  Total pages: 65024                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000] Kernel command line: eQ3Mode=production console=ttyAMA0,115200 ubi.mtd=7 ubi.mtd=6 ro ip=none root=ubi0:root ubi.mtd=7 rootfstype=ubifs noinitrd mtdparts=gpmi-
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] PID hash table entries: 1024 (order: 0, 4096 bytes)                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] Dentry cache hash table entries: 32768 (order: 5, 131072 bytes)                                        
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] Inode-cache hash table entries: 16384 (order: 4, 65536 bytes)                                          
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] allocated 524288 bytes of page_cgroup                                                                  
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] please try 'cgroup_disable=memory' option if you don't want memory cgroups
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] Memory: 256MB = 256MB total                                                                                                                                      
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000] Memory: 255332k/255332k available, 6812k reserved, 0K highmem                                                                                                  
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000] Virtual kernel memory layout:                                                                                                                                  
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]     vector  : 0xffff0000 - 0xffff1000   (   4 kB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]     fixmap  : 0xfff00000 - 0xfffe0000   ( 896 kB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]     vmalloc : 0xd0800000 - 0xff000000   ( 744 MB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]     lowmem  : 0xc0000000 - 0xd0000000   ( 256 MB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]     modules : 0xbf000000 - 0xc0000000   (  16 MB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]       .text : 0xc0008000 - 0xc036f000   (3484 kB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]       .init : 0xc036f000 - 0xc038c000   ( 116 kB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]       .data : 0xc038c000 - 0xc03b67a0   ( 170 kB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.000000]        .bss : 0xc03b67c4 - 0xc03e92bc   ( 203 kB)                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] SLUB: Genslabs=13, HWalign=32, Order=0-3, MinObjects=0, CPUs=1, Nodes=1                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] NR_IRQS:304                                                                                                                                                      
Dec 13 10:35:25 homematic-ccu2 user.err kernel: [    0.000000] saif0_clk_set_rate: clock is gated                                                                                                                                
Dec 13 10:35:25 homematic-ccu2 user.err kernel: [    0.000000] saif1_clk_set_rate: clock is gated                                                                                                                                
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] sched_clock: 32 bits at 100 Hz, resolution 10000000ns, wraps every 4294967286ms                                                                                  
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] Console: colour dummy device 80x30                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.000000] Calibrating delay loop... 226.09 BogoMIPS (lpj=1130496)                                                
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] pid_max: default: 32768 minimum: 301                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] Mount-cache hash table entries: 512                                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] Initializing cgroup subsys cpuacct                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] Initializing cgroup subsys memory
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] Initializing cgroup subsys devices                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] Initializing cgroup subsys freezer                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] CPU: Testing write buffer coherency: ok                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] Setting up static identity map for 0x402a5098 - 0x402a50f0                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.070000] devtmpfs: initialized                                                                                                                                            
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.080000] dummy:                                                                                                                                                           
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.080000] NET: Registered protocol family 16                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.080000] gpiochip_add: registered GPIOs 0 to 31 on device: gpio-mxs.0                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.080000] gpiochip_add: registered GPIOs 32 to 63 on device: gpio-mxs.1                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.080000] gpiochip_add: registered GPIOs 64 to 95 on device: gpio-mxs.2                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.080000] gpiochip_add: registered GPIOs 96 to 127 on device: gpio-mxs.3                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.080000] gpiochip_add: registered GPIOs 128 to 159 on device: gpio-mxs.4                                                                                                  
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.090000] Serial: AMBA PL011 UART driver                                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.090000] duart: ttyAMA0 at MMIO 0x80074000 (irq = 47) is a PL011 rev2                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.100000] console [ttyAMA0] enabled                                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.100000] mxs-usbphy mxs-usbphy.0: initialized usb phy                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.110000] mxs-usbphy mxs-usbphy.1: initialized usb phy                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.120000] bio: create slab <bio-0> at 0                                                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.130000] mxs-dma mxs-dma-apbh: initialized                                                                      
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.140000] mxs-dma mxs-dma-apbx: initialized                                                                      
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.140000] REG-3V3: 3300 mV normal                                                                                
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.150000] REG-1V8: 1800 mV normal                                                                                
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.150000] USB 5V: 5000 mV normal
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.150000] VDDIO-SD: 3300 mV normal                                                                                                                                         
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.160000] Switching to clocksource mxs_timer                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.200000] NET: Registered protocol family 2                                                                                                                                
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.200000] IP route cache hash table entries: 2048 (order: 1, 8192 bytes)                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.210000] TCP established hash table entries: 8192 (order: 4, 65536 bytes)                                                                                                 
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.220000] TCP bind hash table entries: 8192 (order: 3, 32768 bytes)                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.220000] TCP: Hash tables configured (established 8192 bind 8192)                                                                                                         
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.230000] TCP: reno registered                                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.230000] UDP hash table entries: 256 (order: 0, 4096 bytes)                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.240000] UDP-Lite hash table entries: 256 (order: 0, 4096 bytes)                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.250000] NET: Registered protocol family 1                                                                                                                                
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.250000] RPC: Registered named UNIX socket transport module.                                                                                                              
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.260000] RPC: Registered udp transport module.                                                                                                                            
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.260000] RPC: Registered tcp transport module.                                                                                                                            
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.270000] RPC: Registered tcp NFSv4.1 backchannel transport module.                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.280000] audit: initializing netlink socket (disabled)                                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.280000] type=2000 audit(0.280:1): initialized                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.490000] msgmni has been set to 498                                                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.500000] Block layer SCSI generic (bsg) driver version 0.4 loaded (major 251)                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.500000] io scheduler noop registered (default)                                                                 
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.510000] uart-pl011 duart: no DMA platform data                                                                 
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.510000] mxs-auart.0: ttyAPP0 at MMIO 0x8006a000 (irq = 112) is a mxs-auart.0                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.520000] mxs-auart mxs-auart.0: Found APPUART 3.1.0
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.540000] NAND device: Manufacturer ID: 0xec, Chip ID: 0xda (Samsung NAND 256MiB 3,3V 8-bit)                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    0.550000] Scanning device for bad blocks                                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.580000] Bad eraseblock 132 at 0x000001080000                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.720000] Bad eraseblock 808 at 0x000006500000                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.790000] Bad eraseblock 1135 at 0x000008de0000                                                                                                                            
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.910000] Bad eraseblock 1709 at 0x00000d5a0000                                                                                                                            
Dec 13 10:35:25 homematic-ccu2 user.warn kernel: [    0.970000] Bad eraseblock 1970 at 0x00000f640000                                                                                                                            
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.990000] 8 cmdlinepart partitions found on MTD device gpmi-nand                                                                                                         
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    0.990000] Creating 8 MTD partitions on "gpmi-nand":                                                                                                                      
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.000000] 0x000000000000-0x000000100000 : "fcb"                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.000000] 0x000000100000-0x000000200000 : "bbt"                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.010000] 0x000000200000-0x000000300000 : "bootenv"                                                                                                                      
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.020000] 0x000000300000-0x000000480000 : "bootstream0"                                                                                                                  
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.030000] 0x000000480000-0x000000a80000 : "bootstream1"                                                                                                                  
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.040000] 0x000000a80000-0x000000e80000 : "kernel"                                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.050000] 0x000000e80000-0x000003e80000 : "user"                                                                                                                         
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.050000] 0x000003e80000-0x000010000000 : "root"                                                                                                                         
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    1.060000] GPMI NAND driver registered. (IMX)                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.070000] UBI: attaching mtd7 to ubi0                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.070000] UBI: physical eraseblock size:   131072 bytes (128 KiB)                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.080000] UBI: logical eraseblock size:    126976 bytes                                                        
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.080000] UBI: smallest flash I/O unit:    2048                                                                
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.090000] UBI: VID header offset:          2048 (aligned 2048)
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    1.100000] UBI: data offset:                4096                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.810000] UBI: max. sequence number:       7                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.840000] UBI: attached mtd7 to ubi0                                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.840000] UBI: MTD device name:            "root"                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.840000] UBI: MTD device size:            193 MiB                                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.850000] UBI: number of good PEBs:        1544                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.850000] UBI: number of bad PEBs:         4                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.860000] UBI: number of corrupted PEBs:   0                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.860000] UBI: max. allowed volumes:       128                                                                                                                           
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.870000] UBI: wear-leveling threshold:    4096                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.870000] UBI: number of internal volumes: 1                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.880000] UBI: number of user volumes:     1                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.880000] UBI: available PEBs:             0                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.890000] UBI: total number of reserved PEBs: 1544                                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.890000] UBI: number of PEBs reserved for bad PEB handling: 15                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.900000] UBI: max/mean erase counter: 3/1                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.900000] UBI: image sequence number:  350665523                                                                                                                         
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.910000] UBI: background thread "ubi_bgt0d" started, PID 32                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.910000] UBI: attaching mtd6 to ubi1                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.920000] UBI: physical eraseblock size:   131072 bytes (128 KiB)                                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.920000] UBI: logical eraseblock size:    126976 bytes                                                        
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.930000] UBI: smallest flash I/O unit:    2048                                                                
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.930000] UBI: VID header offset:          2048 (aligned 2048) 
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    2.940000] UBI: data offset:                4096                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.370000] UBI: max. sequence number:       257                                                                                                                           
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.390000] UBI: attached mtd6 to ubi1                                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.390000] UBI: MTD device name:            "user"                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.400000] UBI: MTD device size:            48 MiB                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.400000] UBI: number of good PEBs:        383                                                                                                                           
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.410000] UBI: number of bad PEBs:         1                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.410000] UBI: number of corrupted PEBs:   0                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.420000] UBI: max. allowed volumes:       128                                                                                                                           
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.420000] UBI: wear-leveling threshold:    4096                                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.420000] UBI: number of internal volumes: 1                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.430000] UBI: number of user volumes:     1                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.430000] UBI: available PEBs:             0                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.440000] UBI: total number of reserved PEBs: 383                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.440000] UBI: number of PEBs reserved for bad PEB handling: 3                                                                                                           
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.450000] UBI: max/mean erase counter: 2/1                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.450000] UBI: image sequence number:  2047575981                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.460000] UBI: background thread "ubi_bgt1d" started, PID 33                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.err kernel: [    3.460000] UBI error: ubi_init: cannot attach mtd7                                                                 
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.500000] fec_enet_mii_bus: probed                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.510000] rtc-rs5c372 0-0032: rs5c372a found, 24hr, driver version 0.6                                           
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.520000] rtc-rs5c372 0-0032: rtc core: registered rtc-rs5c372 as rtc0                                           
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.530000] stmp3xxx-rtc stmp3xxx-rtc: rtc core: registered stmp3xxx-rtc as rtc1
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.550000] cpuidle: using governor ladder                                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.550000] cpuidle: using governor menu                                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    3.550000] Registered led device: power                                                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    3.550000] Registered led device: internet                                                                                                                                 
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    3.560000] Registered led device: info                                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.560000] NET: Registered protocol family 17                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.560000] registered taskstats version 1                                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.570000] rtc-rs5c372 0-0032: setting system clock to 2015-12-13 09:35:23 UTC (1449999323)                                                                                 
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.690000] UBIFS: mounted UBI device 0, volume 0, name "root"                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.690000] UBIFS: mounted read-only                                                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.690000] UBIFS: file system size:   192241664 bytes (187736 KiB, 183 MiB, 1514 LEBs)                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.700000] UBIFS: journal size:       9023488 bytes (8812 KiB, 8 MiB, 72 LEBs)                                                                                            
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.710000] UBIFS: media format:       w4/r0 (latest is w4/r0)                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.720000] UBIFS: default compressor: lzo                                                                                                                                 
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    3.720000] UBIFS: reserved for root:  0 bytes (0 KiB)                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.730000] VFS: Mounted root (ubifs filesystem) readonly on device 0:12.                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.740000] devtmpfs: mounted                                                                                                                                                
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    3.740000] Freeing init memory: 116K                                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    4.340000] UBIFS: mounted UBI device 1, volume 0, name "user"                                                   
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    4.340000] UBIFS: file system size:   46346240 bytes (45260 KiB, 44 MiB, 365 LEBs)                              
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    4.350000] UBIFS: journal size:       9023488 bytes (8812 KiB, 8 MiB, 72 LEBs)                                  
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    4.360000] UBIFS: media format:       w4/r0 (latest is w4/r0)                                                   
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    4.360000] UBIFS: default compressor: lzo
Dec 13 10:35:25 homematic-ccu2 user.notice kernel: [    4.370000] UBIFS: reserved for root:  0 bytes (0 KiB)                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.010000] eq3spi eq3spi.0: master is unqueued, this is deprecated                                                                                                          
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.080000] input: gpio-keys as /devices/platform/gpio-keys/input/input0                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.140000] Freescale High-Speed USB SOC Device Controller driver (Apr 20, 2007)                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    5.150000] mxs-usbphy mxs-usbphy.0: enabling gadget mode                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.230000] usb0: MAC 00:1a:22:00:05:87                                                                                                                                      
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.230000] usb0: HOST MAC 00:1a:22:00:05:86                                                                                                                                 
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.240000] g_multi gadget: Mass Storage Function, version: 2009/09/11                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.250000] g_multi gadget: Number of LUNs=1                                                                                                                                 
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.250000]  lun0: LUN: read only CD-ROM file: /usr/share/eq3/install.iso                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.260000] g_multi gadget: Multifunction Composite Gadget                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.270000] g_multi gadget: g_multi ready                                                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.270000] fsl-usb2-udc: bind to driver g_multi                                                                                                                             
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.300000] tun: Universal TUN/TAP device driver, 1.6                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.310000] tun: (C) 1999-2004 Max Krasnyansky <maxk@qualcomm.com>                                                                                                           
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.400000] usbcore: registered new interface driver usbfs                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.410000] usbcore: registered new interface driver hub                                                                                                                     
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.410000] usbcore: registered new device driver usb                                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.440000] ehci_hcd: USB 2.0 'Enhanced' Host Controller (EHCI) Driver                                             
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.450000] mxs-ehci mxs-ehci.1: initializing i.MX USB Controller                                                  
Dec 13 10:35:25 homematic-ccu2 user.debug kernel: [    5.460000] mxs-usbphy mxs-usbphy.1: enabling host mode                                                           
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.480000] mxs-ehci mxs-ehci.1: using regulator to control VBUS                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.480000] mxs-ehci mxs-ehci.1: Freescale On-Chip EHCI Host Controller

Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.490000] mxs-ehci mxs-ehci.1: new USB bus registered, assigned bus number 1                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.530000] mxs-ehci mxs-ehci.1: irq 92, io mem 0x80090000                                                                                                                   
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.550000] mxs-ehci mxs-ehci.1: USB 2.0 started, EHCI 1.00                                                                                                                  
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.550000] usb usb1: New USB device found, idVendor=1d6b, idProduct=0002                                                                                                    
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.560000] usb usb1: New USB device strings: Mfr=3, Product=2, SerialNumber=1                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.570000] usb usb1: Product: Freescale On-Chip EHCI Host Controller                                                                                                        
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.570000] usb usb1: Manufacturer: Linux 3.4.11.ccu2 ehci_hcd                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.580000] usb usb1: SerialNumber: mxs-ehci.1                                                                                                                               
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.580000] hub 1-0:1.0: USB hub found                                                                                                                                       
Dec 13 10:35:25 homematic-ccu2 user.info kernel: [    5.590000] hub 1-0:1.0: 1 port detected                                                                                                                                     
Dec 13 10:35:26 homematic-ccu2 user.err kernel: 0>[    6.120000] udevd[101]: starting version 182                                                                                                                                
Dec 13 09:35:26 homematic-ccu2 daemon.err udevd[101]: specified group 'dialout' unknown                                                                                                                                          
Dec 13 09:35:26 homematic-ccu2 daemon.err udevd[101]: specified group 'kmem' unknown                                                                                                                                             
Dec 13 09:35:26 homematic-ccu2 daemon.err udevd[101]: specified group 'video' unknown                                                                                                                                            
Dec 13 09:35:26 homematic-ccu2 daemon.err udevd[101]: specified group 'lp' unknown                                                                                                                                               
Dec 13 09:35:26 homematic-ccu2 daemon.err udevd[101]: specified group 'floppy' unknown                                                                                                                                           
Dec 13 09:35:26 homematic-ccu2 daemon.err udevd[101]: specified group 'cdrom' unknown                                                                                                                                            
Dec 13 09:35:26 homematic-ccu2 daemon.err udevd[101]: specified group 'tape' unknown                                                                                                                                             
Dec 13 10:35:27 homematic-ccu2 user.info kernel: [    7.550000] mxs-mmc mxs-mmc.0: using regulator to control VDDIO-SD                                                 
Dec 13 10:35:27 homematic-ccu2 user.info kernel: [    7.600000] mxs-mmc mxs-mmc.0: initialized                                                                         
Dec 13 10:35:27 homematic-ccu2 daemon.info udhcpd[137]: udhcpd (v1.20.2) started                                                                                       
Dec 13 10:35:27 homematic-ccu2 daemon.err udhcpd[137]: can't open '/var/lib/misc/udhcpd.leases': No such file or directory                                             
Dec 13 09:35:28 homematic-ccu2 daemon.info ifplugd(eth0)[181]: ifplugd 0.28 initializing.
Dec 13 10:35:28 homematic-ccu2 user.info kernel: [    9.040000] eth0: Freescale FEC PHY driver [SMSC LAN8710/LAN8720] (mii_bus:phy_addr=imx28-fec-1:00, irq=185)                                                                 
Dec 13 09:35:28 homematic-ccu2 daemon.info ifplugd(eth0)[181]: Using interface eth0/00:1A:22:04:D6:3A with driver <fec> (version: Revision: 1.0)                                                                                 
Dec 13 09:35:28 homematic-ccu2 daemon.info ifplugd(eth0)[181]: Using detection mode: SIOCETHTOOL                                                                                                                                 
Dec 13 09:35:28 homematic-ccu2 daemon.info ifplugd(eth0)[181]: Initialization complete, link beat not detected.                                                                                                                  
Dec 13 10:35:30 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:35:30 homematic-ccu2 user.debug setclock: Sun Dec 13 10:35:30 CET 2015                                                                                                                                                 
Dec 13 10:35:30 homematic-ccu2 user.info kernel: [   11.040000] PHY: imx28-fec-1:00 - Link is Up - 100/Full                                                                                                                      
Dec 13 09:35:31 homematic-ccu2 daemon.info ifplugd(eth0)[181]: Link beat detected.                                                                                                                                               
Dec 13 09:35:31 homematic-ccu2 auth.info sshd[226]: Server listening on 0.0.0.0 port 22.                                                                                                                                         
Dec 13 09:35:32 homematic-ccu2 daemon.info ifplugd(eth0)[181]: Executing '/etc/ifplugd/ifplugd.action eth0 up'.                                                                                                                  
Dec 13 09:35:32 homematic-ccu2 daemon.warn ifplugd(eth0)[181]: client: eth0 carrier detected                                                                                                                                     
Dec 13 09:35:33 homematic-ccu2 user.info logger: Updating RF Lan Gateway Coprocessor Firmware                                                                                                                                    
Dec 13 09:35:33 homematic-ccu2 user.debug update-coprocessor: firmware filename is: coprocessor_update.eq3                                                                                                                       
Dec 13 09:35:33 homematic-ccu2 user.info logger: Updating RF Lan Gateway Firmware                                                                                                                                                
Dec 13 09:35:33 homematic-ccu2 user.info update-lgw-firmware: No gateway found in config file /etc/config/rfd.conf                                                                                                               
Dec 13 09:35:33 homematic-ccu2 user.info logger: Updating Wired Lan Gateway Firmware                                                                                                                                             
Dec 13 09:35:33 homematic-ccu2 user.info update-lgw-firmware: No gateway found in config file /etc/config/hs485d.conf                                                                                                            
Dec 13 10:35:35 homematic-ccu2 user.info update-coprocessor: Version: 1.4.1                                                                                                                                                      
Dec 13 10:35:35 homematic-ccu2 user.info update-coprocessor: No update necessary                                                                                       
Dec 13 09:35:37 homematic-ccu2 daemon.info ifplugd(eth0)[181]: Program executed successfully.                                                                          
Dec 13 10:36:30 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                             
Dec 13 10:37:10 homematic-ccu2 user.debug setclock: Sun Dec 13 10:37:10 CET 2015                                                                                       
Dec 13 10:37:51 homematic-ccu2 user.info : hss_lcd: Programm initialisiert.        
Dec 13 09:37:52 homematic-ccu2 daemon.info init: starting pid 393, tty '/dev/ttyAMA0': '/sbin/getty -L ttyAMA0 115200 vt100 '                                                                                                    
Dec 13 09:37:52 homematic-ccu2 daemon.info init: starting pid 394, tty '/dev/ttyGS0': '/sbin/getty -L ttyGS0 115200 vt100 '                                                                                                      
Dec 13 10:38:10 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:38:24 homematic-ccu2 user.err : node is empty                                                                                                                                                                          
Dec 13 10:38:50 homematic-ccu2 user.debug setclock: Sun Dec 13 10:38:50 CET 2015                                                                                                                                                 
Dec 13 10:39:50 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:40:30 homematic-ccu2 user.debug setclock: Sun Dec 13 10:40:30 CET 2015                                                                                                                                                 
Dec 13 10:41:30 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:42:11 homematic-ccu2 user.debug setclock: Sun Dec 13 10:42:11 CET 2015                                                                                                                                                 
Dec 13 10:43:11 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:43:50 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 10:43:51 homematic-ccu2 user.debug setclock: Sun Dec 13 10:43:51 CET 2015                                                                                                                                                 
Dec 13 10:44:51 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:45:30 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 10:45:31 homematic-ccu2 user.debug setclock: Sun Dec 13 10:45:31 CET 2015                                                                                                                                                 
Dec 13 10:46:31 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:47:10 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 10:47:11 homematic-ccu2 user.debug setclock: Sun Dec 13 10:47:11 CET 2015                                                                                                                                                 
Dec 13 10:48:11 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                             
Dec 13 10:48:51 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]
Dec 13 10:48:51 homematic-ccu2 user.debug setclock: Sun Dec 13 10:48:51 CET 2015                                                                                       
Dec 13 10:49:51 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                             
Dec 13 10:50:31 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]

Dec 13 10:50:31 homematic-ccu2 user.debug setclock: Sun Dec 13 10:50:31 CET 2015                                                                                                                                                 
Dec 13 10:51:31 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:52:11 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 10:52:12 homematic-ccu2 user.debug setclock: Sun Dec 13 10:52:12 CET 2015                                                                                                                                                 
Dec 13 10:53:12 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:53:51 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 10:53:52 homematic-ccu2 user.debug setclock: Sun Dec 13 10:53:52 CET 2015                                                                                                                                                 
Dec 13 10:54:52 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:55:31 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 10:55:32 homematic-ccu2 user.debug setclock: Sun Dec 13 10:55:32 CET 2015                                                                                                                                                 
Dec 13 10:56:32 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:57:11 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 10:57:12 homematic-ccu2 user.debug setclock: Sun Dec 13 10:57:12 CET 2015                                                                                                                                                 
Dec 13 10:58:12 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 10:58:51 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 10:58:52 homematic-ccu2 user.debug setclock: Sun Dec 13 10:58:52 CET 2015                                                                                                                                                 
Dec 13 10:59:52 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 11:00:32 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 11:00:32 homematic-ccu2 user.debug setclock: Sun Dec 13 11:00:32 CET 2015                                                                                       
Dec 13 11:01:32 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                             
Dec 13 11:02:12 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]
Dec 13 11:02:13 homematic-ccu2 user.debug setclock: Sun Dec 13 11:02:13 CET 2015                                                                                       
Dec 13 11:03:13 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com   
Dec 13 11:03:52 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 11:03:53 homematic-ccu2 user.debug setclock: Sun Dec 13 11:03:53 CET 2015                                                                                                                                                 
Dec 13 11:04:53 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 11:05:32 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 11:05:33 homematic-ccu2 user.debug setclock: Sun Dec 13 11:05:33 CET 2015                                                                                                                                                 
Dec 13 11:06:33 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 11:07:12 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 11:07:13 homematic-ccu2 user.debug setclock: Sun Dec 13 11:07:13 CET 2015                                                                                                                                                 
Dec 13 11:08:13 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 11:08:52 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 11:08:53 homematic-ccu2 user.debug setclock: Sun Dec 13 11:08:53 CET 2015                                                                                                                                                 
Dec 13 11:09:53 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 11:10:32 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 11:10:33 homematic-ccu2 user.debug setclock: Sun Dec 13 11:10:33 CET 2015                                                                                                                                                 
Dec 13 11:11:34 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 11:12:12 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]                                                          
Dec 13 11:12:14 homematic-ccu2 user.debug setclock: Sun Dec 13 11:12:14 CET 2015                                                                                                                                                 
Dec 13 11:13:14 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                                                                                       
Dec 13 11:13:53 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]
Dec 13 11:13:54 homematic-ccu2 user.debug setclock: Sun Dec 13 11:13:54 CET 2015                                                                                       
Dec 13 11:14:54 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                             
Dec 13 11:15:33 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]
Dec 13 11:15:34 homematic-ccu2 user.debug setclock: Sun Dec 13 11:15:34 CET 2015       
Dec 13 11:16:34 homematic-ccu2 user.debug setclock: Try to get time from ntp.homematic.com                                                                             
Dec 13 10:17:10 homematic-ccu2 auth.info sshd[750]: Accepted password for root from 192.168.1.124 port 62161 ssh2                                                      
Dec 13 11:17:13 homematic-ccu2 local0.emerg ReGaHss: Crash: Could not spawn a new request handler! {"HTTP-Listener"} [../Platform/Internet/http/httpListener.cpp (175)]
Dec 13 11:17:14 homematic-ccu2 user.debug setclock: Sun Dec 13 11:17:14 CET 2015